<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle>
    <drawing>
        <library name="Upverter Library">
            <description>Upverter Parts Library

Created by Upverter.com</description>
            <packages>
                <package name="TEXAS_INSTRUMENTS_UA723CDR_0">
                    <description></description>
                </package>
            </packages>
            <symbols>
                <symbol name="TEXAS_INSTRUMENTS_UA723CDR_0_0">
                    <description></description>
                    <pin name="VCC+"/>
                    <pin name="VCC–"/>
                    <pin name="CURR_LIM"/>
                    <pin name="CURR_SENS"/>
                    <pin name="IN+"/>
                    <pin name="IN–"/>
                    <pin name="FREQ_COMP"/>
                    <pin name="OUTPUT"/>
                    <pin name="REF"/>
                    <pin name="VC"/>
                    <pin name="VZ"/>
                    <pin name="NC"/>
                    <pin name="NC2"/>
                    <pin name="NC3"/>
                </symbol>
            </symbols>
            <devicesets>
                <deviceset prefix="U" name="TEXAS_INSTRUMENTS_UA723CDR">
                    <description></description>
                    <gates>
                        <gate name="G$0" symbol="TEXAS_INSTRUMENTS_UA723CDR_0_0"/>
                    </gates>
                    <devices>
                        <device name="TEXAS_INSTRUMENTS_UA723CDR_0_0" package="TEXAS_INSTRUMENTS_UA723CDR_0">
                            <connects>
                                <connect gate="G$0" pad="1" pin="NC"/>
                                <connect gate="G$0" pad="2" pin="CURR_LIM"/>
                                <connect gate="G$0" pad="3" pin="CURR_SENS"/>
                                <connect gate="G$0" pad="4" pin="IN–"/>
                                <connect gate="G$0" pad="5" pin="IN+"/>
                                <connect gate="G$0" pad="6" pin="REF"/>
                                <connect gate="G$0" pad="7" pin="VCC–"/>
                                <connect gate="G$0" pad="8" pin="NC2"/>
                                <connect gate="G$0" pad="9" pin="VZ"/>
                                <connect gate="G$0" pad="10" pin="OUTPUT"/>
                                <connect gate="G$0" pad="11" pin="VC"/>
                                <connect gate="G$0" pad="12" pin="VCC+"/>
                                <connect gate="G$0" pad="13" pin="FREQ_COMP"/>
                                <connect gate="G$0" pad="14" pin="NC3"/>
                            </connects>
                            <technologies>
                                <technology>
                                    <attribute name="mouser_part_number" value="595-UA723CDR"/>
                                    <attribute name="centroid_not_specified" value="No"/>
                                    <attribute name="temperature_range_high" value="+70°C"/>
                                    <attribute name="MPN" value="UA723CDR"/>
                                    <attribute name="digikey_description" value="IC Linear Voltage Regulator IC Positive Adjustable 1 Output 2 V ~ 37 V 150mA 14-SOIC"/>
                                    <attribute name="digikey_part_number" value="296-11102-1-ND"/>
                                    <attribute name="prefix" value="U"/>
                                    <attribute name="Current_-_Output" value="150mA"/>
                                    <attribute name="Line_Regulation" value="5 mV / V"/>
                                    <attribute name="lead_free" value="yes"/>
                                    <attribute name="mfg_package_ident" value="D (R-PDSO-G14)"/>
                                    <attribute name="voltage" value="40V"/>
                                    <attribute name="temperature_range_low" value="0°C"/>
                                    <attribute name="rohs" value="yes"/>
                                    <attribute name="datasheet" value="http://www-s.ti.com/sc/ds/ua723.pdf"/>
                                    <attribute name="Voltage_-_Output" value="2 V ~ 37 V"/>
                                    <attribute name="MF" value="Texas Instruments"/>
                                    <attribute name="package" value="SOIC-14"/>
                                </technology>
                            </technologies>
                        </device>
                    </devices>
                </deviceset>
            </devicesets>
        </library>
    </drawing>
</eagle>
